# Viewing VLACP Global information

Use this procedure to view VLACP information for the switch.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the VLACP Global tab.

## Variable definitions

The following table outlines the parameters of the VLACP Global tab.

Table 1. MLT/LACP Global tab VLACP section parameters
Variable | Value
--- | ---
VlacpEnable | Enables or disables VLACP on the switch.
VlacpMulticastMACAddress | Identifies a multicast MAC address used exclusively for VLACPDUs. Default is 01:80:c2:00:11:00.
VlacpHoldTime | Time in seconds after restart to send PDUs with subtype HOLD. Used only when SMLT is enabled. Default is 0.