# Enabling VoIP VLAN using EDM

Use the following procedure to activate the VoIP VLAN.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click 802.1X/EAP.

3. In the work area, click the EAP VoIP Vlan tab.

4. In the table, double-click the cell under the column header you want to edit.

5. Select a parameter or value from the drop-down list.

   You can repeat the previous two steps until you have amended all of the parameters you want to change.

6. On the toolbar, click Apply.

## Variable Definitions

The following table defines variables you can use to enable VoIP VLAN.

Variable | Value
--- | ---
MultiHostVoipVlanIndex | Indicates the multihost VoIP VLAN index. The range is 1–5.
MultiHostVoipVlanEnabled | Enables (true) or disables (false) the multihost VoIP VLAN.
MultiHostVoipVlanId | Indicates the VLAN ID; value ranges from 1–4094.