# Viewing LLDP local system properties

Use this procedure to view LLDP local system properties.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Local System tab.

The following table outlines the parameters of the Local System tab.

Table 1. Variable definitions
Variable | Value
--- | ---
ChassisIdSubtype | Specifies the type of encoding used to identify the local system chassis: chassisComponent interfaceAlias portComponent macAddress networkAddress interfaceName local
ChassisId | Specifies the chassis ID
SysName | Specifies the local system name
SysDesc | Specifies the local system description
SysCapSupported | Identifies the system capabilities supported on the local system
SysCapEnabled | Identifies the system capabilities that are enabled on the local system
DeviceClass | Specifies the local MED device class
HardwareRev | Specifies the vendor-specific hardware revision string as advertised by the local device
FirmwareRev | Specifies the vendor-specific firmware revision string as advertised by the local device
SoftwareRev | Specifies the vendor-specific software revision string as advertised by the local device
SerialNum | Specifies the vendor-specific serial number as advertised by the local device
MfgName | Specifies the vendor-specific manufacturer name as advertised by the local device
ModelName | Specifies the vendor-specific model name as advertised by the local device
AssetID | Specifies the vendor-specific asset tracking identifier as advertised by the local device
DeviceType | Defines the type of Power-via-MDI (Power over Ethernet) advertised by the local device: pseDevice: indicates that the device is advertised as a Power Sourcing Entity (PSE). pdDevice: indicates that the device is advertised as a Powered Device (PD) none: indicates that the device does not support PoE
PSEPowerSource | Defines the type of PSE Power Source advertised by the local device: primary: indicates that the device advertises its power source as primary backup: indicates that the device advertises its power source as backup
PDPowerReq | Specifies the value of the power required (in units of 0.1 watts) by a Powered Device (PD)
PDPowerSource | Defines the type of power source advertised as in use by the local device: fromPSE: indicates that the device advertises its power source as received from a PSE local: indicates that the device advertises its power source as local localAndPSE: indicates that the device advertises its power source as using both local and PSE power
PDPowerPriority | Defines the priority advertised as required by this PD: critical: indicates that the device advertises its power priority as critical, see RFC 3621 high: indicates that the device advertises its power priority as high, see RFC 3621 low: indicates that the device advertises its power priority as low, see RFC 3621

Parent topic: LLDP configuration using Enterprise Device Manager