# Viewing LLDP VLAN Name properties

With the Neighbor VLAN Name tab, you can view LLDP VLAN Name properties for the remote system.

To open the Neighbor VLAN Name tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot1.

5. Select the Neighbor VLAN Name tab.

The following table outlines the parameters of the Port dot1 Neighbor VLAN Name tab.

Table 1. PVariable definitions
Vaiable | Value
--- | ---
TimeMark | The TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | An arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
VlanId | The integer value used to identify the IEEE 802.1Q VLAN IDs with which the remote port is compatible.
VlanName | The VLAN name identified by the VLAN ID associated with the remote system.