# Viewing priority mapping

Use this procedure to open the Priority Mapping tab.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Devices.

3. Select the Priority Mapping tab.

## Variable definitions

The following table outlines the parameters of the Priority Mapping tab.

Table 1. QoS Devices Priority Mapping tab parameters
Variable | Value
--- | ---
802.1pPriority | Specifies the 802.1 user priority value to map to a DSCP value at ingress.
Dscp | Specifies the DSCP value to associate with the specified 802.1 user priority value at ingress. To change a DSCP assignment, double-click in a Dscp cell and edit the value.
Name | Specifies the type of service.