# Mapping the LACP key mapping

Use this procedure to map the LACP key mapping.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the LACP key mapping tab.

## Variable definitions

The following table outlines the parameters of the LACP key mapping tab.

Table 1. MLT/LACP LACP key mapping tab parameters
Variable | Value
--- | ---
LacpKeyValue | Specifies the value of the LACP administration key.
MltId | Specifies the ID of the MLT.
SmltId | Specifies the ID of the SMLT.