# Configuring ADAC MAC address ranges using EDM

Use this procedure to add MAC address ranges to the ADAC MAC address range table.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, click ADAC.

3. Select the ADAC MAC Ranges tab.

4. Click Insert.

5. In the MacAddrRangeLowEndIndex field, enter the low-end of the MAC address range to add.

6. In the MacAddrRangeHighEndIndex field, enter the high-end of the MAC address range to add.

7. Click Insert.

The following table outlines the parameters of the ADAC MAC Ranges tab.

Table 1. Variable definitions
Variable | Value
--- | ---
MacAddrRangeLowEndIndex | The MAC address for the low end of the MAC address range.
MacAddrRangeHighEndIndex | The MAC address for the high end of the MAC address range.