# Configuring QoS for the NSNA solution using EDM

Use the following procedure to configure QoS for the NSNA solution using EDM.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

For general information about configuring filters and Quality of Service (QoS) in the NSNA solution, see Filters in the NSNA solution.

For detailed information about configuring the filters, see Avaya Ethernet Routing Switch 5000 Series Configuration — Quality of Service, NN47200-504.