# Filtering an NSNA VLAN

Use this procedure to filter an NSNA VLAN.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click VLANs.

3. Select the NSNA tab.

4. Click Filter.

5. Set the filter parameters.

6. Click Filter.

## Variable definitions

The following table outlines the parameters of the MAC Multicast Filter Table tab.

Table 1. MAC Multicast Filter Table tab parameters
Variable | Value
--- | ---
AllowedAddressVlanId | Specifies the allowed address of the VLAN ID.
AllowedAddressMacAddr | Specifies the allowed address for the MAC address.