# Config/Image/Diag file tab field descriptions job aid

For more information about fields on the Config/Image/Diag file tab, see the following table.

Field name | Description
--- | ---
TftpServerInetAddressType | Specifies the IP version of the TFTP server address
TftpServerInetAddress | Specifies the TFTP server IP address
BinaryConfigFilename | Specifies the name of the binary configuration file
BinaryConfigUnitNumber | Specifies the unit number of a switch in a stack
ImageFileName | Specifies the software image file name
FWFileName(Diagnostics) | Specifies the diagnostics file name
USBTargetUnit | Specifies the unit number containing the USB port
Image | Specifies either primary or secondary when used in conjunction with the dnldImg action.
Action | dnldConfigFromUSB—download a configuration to the switch from a USB device dnldImgIfNewer—download a new software image to the switch only if it is newer than the current image dnldFw—download a new diagnostic software image to the switch dnldConfig—download a configuration file to the switch upldConfigToUsb—upload a configuration file to a USB device dnldImgNoReset—download a new software image to the switch without a switch reset dnldFwNoReset—download a new diagnostic software image to the switch without a switch reset upldConfig—upload a configuration file to the switch from a designated location dnldImg—download a new software image to the switch dnldImgFromUsb—download a new software image to the switch from a USB device dnldFwFromUsb—download a new diagnostic software image to the switch from a USB device
Status | Displays the status of the most recent action since last switch restart.