# Customizing the ACLI banner

Use this procedure to customize banner that is displayed on the Avaya Command Line (ACLI) Telnet screen.

## Before you begin

Select custom for the ACLI banner type.

## Procedure

1. From the navigation tree, double-click Edit.
2. In the Edit tree, double-click Chassis.
3. In the Chassis tree, click Chassis.
4. In the Chassis work area, click the Custom Banner tab.
5. Select a row (switch), configure as required.
6. On the toolbar, click Apply.
7. On the toolbar, you can click Refresh verify the configuration.

## Variable definitions

The following table describes the variables associated with customizing the ACLI banner.

Variable | Value
--- | ---
Type | Indicates whether the banner type is for a standalone (switch) or a stack (stack).
Id | Indicates the line of text within a custom banner.
Line | Specifies the banner character string. The custom banner is 19 lines high and can be up to 80 characters long.