# Enabling SLPP PDU received function per port

Use this procedure to enable the SLPP PDU received function on a port.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click SLPP.

3. Select the Ports tab.

4. Under the SlppEnable heading, select the port you want to enable.

5. Double click to select True (enabled) or False (disabled).

6. Click Apply.

7. Click Close.