# Configuring Last RADIUS Assigned VLAN on a port using EDM

Use the following procedure to enable or disable Last Assigned VLAN on a port.

## Procedure steps

1. Open one of the supported browsers.

2. Enter the IP address of the switch to open an EDM session.

3. On the Device Physical View, select a port.

4. Right-click the port and double-click Edit.

5. In the work area, click the EAPOL Advance tab.

6. In the work area, select the MultihostUseMostRecentRadiusAssignedVlan option.

7. On the toolbar, click Apply.