# Clearing the MAC address table on a FastEthernet interface

Use the following procedure to flush the MAC addresses for the specified ports. This command does not flush the addresses learned on the trunk.

## Procedure steps

1. TO clear the MAC address table on a FastEthernet interface, use the following command from Privileged EXEC mode.

   `clear mac-address-table interface FastEthernet <port-list|ALL>`