# IGMP snooping configuration using Enterprise Device Manager

This chapter describes the procedures you can use to configure IGMP snooping on a VLAN using Enterprise Device Manager (EDM).

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Configuring IGMP snooping using EDM

1. Enable snoop on the VLAN.

   All related configurations, listed below, are optional and can be configured to suit the requirements of your network.