# Viewing SNMP information using EDM

Use the SNMP tab to display read-only information about the addresses that the agent software uses to identify the switch.

Use the following procedure to view the SNMP information.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Chassis.

3. In the Chassis tree, double-click Chassis.

4. In the work area, click the SNMP tab to view SNMP information.

## Variable definitions

The following table describes the fields of SNMP tab.

Variable | Value
--- | ---
LastUnauthenticatedInetAddressType | Specifies the type of IP address that was not authenticated by the device last.
LastUnauthenticatedInetAddress | Specifies the last IP address that was not authenticated by the device.
LastUnauthenticatedCommunityString | Specifies the last community string that was not authenticated by the device.
RemoteLoginInetAddressType | Specifies the type of IP address to last remotely log on to the system.
RemoteLoginInetAddress | Specifies the last IP address to remotely log on to the system.
TrpRcvrMaxEnt | Specifies the maximum number of trap receiver entries.
TrpRcvrCurEnt | Specifies the current number of trap receiver entries.
TrpRcvrNext | Specifies the next trap receiver entry to be created.