# Configuring host notification control using EDM

Use the following procedure to configure host notification controls.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Snmp Server.

3. In the Snmp Server tree, double-click Host.

4. In the work area, select a host.

5. In the toolbar, click Notification.

   The Host Notification Control tab appears.

6. In the work area, select the notifications you want to enable.

   OR

   In the toolbar, click Enable All to enable all the notifications.

   OR

   In the toolbar, click Disable All to disable all the notifications.

7. In the toolbar, click Apply.

## Variable definitions

The following table describes the fields of Host Notification Controls tab.

Variable | Value
--- | ---
coldStart | Signifies that the SNMPv2 entity, acting in an agent role, is reinitializing itself, and that its configuration may for each altered.
warmStart | Signifies that the SNMPv2 entity, acting in an agent role, is reinitializing itself such that its configuration is unaltered.
linkDown | Signifies that the SNMPv2 entity, acting in an agent role, has detected that the ifOperStatus object for one of its communication links is about to transition into the down state.
linkUp | Signifies that the SNMPv2 entity, acting in an agent role, has detected that the ifOperStatus object for one of its communication links has come out of the down state.
authenticationFailure | Signifies that the SNMP entity has received a protocol message that is not properly authenticated.
s5EtrSbsMacTableFull | Signifies that the mac-security address table is filled.
s5EtrSbsMacTableClearedForPort | Signifies that the mac-security address table is cleared for a particular port.
s5EtrSbsMacTableCleared | Signifies that the mac-security address table is cleared for all ports.
s5EtrSbsMacRemoved | Signifies that a mac address is removed from the mac-security address table.
s5EtrNewSbsMacAccessViolation | Signifies a trap is sent when the switch device detects a Mac_address based security violation on a port set by s5SbsSecurityAction defined in s5sbs100.mib. This trap is sent only once, when the condition is first detected.
s5CtrNewHotSwap | Signifies that a component or sub component is inserted or removed from chassis. This trap is sent only once when the condition is first detected.
s5CtrNewProblem | Signifies that a component or sub component has a problem like warning, nonfatal, or fatal. This trap is sent only once when the condition is first detected.
s5CtrNewUnitUp | Signifies that a component or sub component is newly detected. This trap is sent only once when the condition is first detected.
s5CtrNewUnitDown | Signifies that a component or sub component is no longer detected. This trap is sent only once when the condition is first detected.
bsAdacPortConfigNotification | Signifies that whether the Auto-Configuration is applied or not on the port. This trap is sent on every status change.
bsAdacPortOperDisabledNotification | Indicates whether a port having bsAdacPortAdminEnable set to true changes its bsAdacPortOperEnable from true to false due to some condition such as reaching the maximum number of devices supported for each port.
bsveVrrpTrapStateTransition | Signifies that a state transition has occurred on a particular vrrp interface. Implementation of this trap is optional.
bsDhcpSnoopingBindingTableFull | Signifies that an attempt is made to add a new DHCP binding entry when the binding table is full.
bsDhcpSnoopingTrap | Signifies that a DHCP packet is dropped.
bsDhcpOption82MaxLengthExceeded | Signifies that the DHCP Option 82 information could not be added to a DHCP packet because the size of the resulting packet is too long.
bsaiArpPacketDroppedOnUntrustedPort | Signifies that an ARP packet is dropped on an untrusted port due to an invalid IP/MAC binding.
bsSourceGuardReachedMaxIpEntries | Signifies that the maximum number of IP entries on a port has been reached.
bsSourceGuardCannotEnablePort | Signifies that there are insufficient resources available to enable IP source guard checking on a port. Important This notification is not generated as the result of a management operation, but rather as a result of internal state changes within the system.
bspimeNeighborStateChanged | Signifies a change of state of an adjacency with a neighbor. This notification is generated when the PIM interface of the router is disabled or enabled, or when a PIM neighbor adjacency of route expires or establishes.
bsnConfigurationSavedToNvram | Signifies that the device saves its configuration to non volatile storage.
bsnEapAccessViolation | Signifies that an EAP access violation occurs.
bsnStackManagerReconfiguration | Stackable system generates this notification when the stack manager detects a problem with a link between stack members.
bsnLacTrunkUnavailable | Signifies that an attempt is made to form an 802.3ad LAG trunk, but there are no available resources to create a new trunk.
bsnLoginFailure | Signifies that an attempt to login to the system fails because of an incorrect password.
bsnTrunkPortDisabledToPrevent BroadcastStorm | Signifies that an MLT port is disabled because an MLT trunk is disabled.
bsnTrunkPortEnabledToPreventBroadcastStorm | Signifies that an MLT port is enabled because an MLT trunk is disabled.
bsnLacPortDisabledDueToLossOfVLACPDU | Signifies that a port is disabled due to the loss of a VLACP PDU.
bsnLacPortEnabledDueToReceiptOfVLACPDU | Signifies that a port is enabled due to receipt of a VLACP PDU.
bsnStackConfigurationError | Signifies that the expected size of a stack is not equal to the actual size of the stack.
bsnEapUbpFailure | Signifies that the installation of a UBP policy fails following EAP authentication.
bsnTrialLicenseExpiration | Signifies that a trial license is going to expire soon, or has already expired.
bsnEnteredForcedStackMode | Signifies that a switch has entered forced stack mode.
bsnEapRAVError | Signifies that the MAC address that was authorized on a port which could not be moved to the Radius-Assigned VLAN.
lldpRemTablesChange | Signifies that the value of lldpStatsRemTableLastChangeTime is changed.
risingAlarm | Signifies that an alarm entry is crossing its rising threshold and generating an event that is configured for sending SNMP traps.
fallingAlarm | Signifies that an alarm entry is crossing its falling threshold and generating an event that is configured for sending SNMP traps.
vrrpTrapNewMaster | Signifies that the sending agent has transitioned to 'Master' state.
pethPsePortOnOffNotification | Indicates if Pse Port is delivering or not power to the PD. This Notification is sent on every status change except in the searching mode.
pethMainPowerUsageOnNotification | Indicate that PSE threshold usage indication is on, and the usage power is above the threshold.
pethMainPowerUsageOffNotification | Indicates that PSE Threshold usage indication is off and the usage power is below the threshold.
ospfVirtIfStateChange | Signifies that the value of ospfVirtIfStateChange is enabled.
ospfNbrStateChange | Signifies that the value of ospfNbrStateChangeis enabled.
ospfVirtNbrStateChange | Signifies that the value of ospfVirtNbrStateChange is enabled.
ospfIfConfigError | Signifies that the value of ospfIfConfigError is enabled.
ospfVirtIfConfigError | Signifies that the value of ospfVirtIfConfigError is enabled.
ospfIfAuthFailure | Signifies that the value of ospfIfAuthFailure is enabled.
ospfVirtIfAuthFailure | Signifies that the value of ospfVirtIfAuthFailureis enabled.
ospfIfStateChange | Signifies that the value of ospfIfStateChange is enabled.
entConfigChange | Signifies that the value of entConfigChangeis enabled.
lldpXMedTopologyChangeDetected | Local device generates this notification when they sense a change in the topology. The change indicates that a new remote device attached to a local port, or a remote device disconnected or moved from one port to another.
ntnQosPolicyEvolLocalUbpSessionFailure | Signifies that filter data associated with a user could not be installed in the context of local UBP support.
ntnQosPolicyEvolDosAttackDetected | Indicates that the DAPP support has detected an attack on the device generating this trap. A notification is generated once for each unit that contains ports on which an attack is detected.
rcnSmltIstLinkUp | Signifies that the split MLT link is from down to up.
rcnSmltIstLinkDown | Signifies that the split MLT link is from up to down.
rcnSmltLinkUp | Signifies that the split SMLT link is up.
rcnSmltLinkDown | Signifies that the split SMLT link is down.
rcnBpduReceived | Signifies that a BPDU is received on a port which has BPDU filtering enabled.
rcnSlppPortDownEventNew | Signifies that a port down event that has occurred due to SLPP.
ubpEAPSessionStart | Signifies start of EAP session.
ubpEAPSessionEnd | Signifies end of EAP session.