# Displaying STG ports

Use this procedure to display the STG port status.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, double-click Spanning Tree.

3. From the Spanning Tree folder, click STG.

4. Select the Ports tab.

## Variable definitions

The following table outlines the parameters of the Ports tab.

Table 1. STG Ports tab parameters
Variable | Value
--- | ---
Port | Indicates the switch position in a stack and port number. For a standalone switch, the default value of 1 is used for the switch position.
StgId | Displays the STG ID number assigned to the port.
Priority | Specifies the port priority
State | Displays the STP state of the port: Disabled, Blocking, Listening, Learning, Forwarding.
EnableStp | Enables or disables STP on the port: True is enabled, and False is disabled.
FastStart | Enables or disables Fast Start STP on the port: True is enabled, and False is disabled.
AdminPathCost | Sets the PathCost value. The field displays 0 if no user-configured value exists.
PathCost | Displays the contribution of this port to the cost path of the spanning tree root.
DesignatedRoot | Displays the MAC address of the STP designated root.
DesignatedCost | Displays the path cost of the designated port of the segment connected to this port.
DesignatedBridge | Displays the MAC address of the designated bridge this port considers the designated bridge for this segment.
DesignatedPort | Displays the port ID of the designated bridge for this port segment.
ForwardTransitions | Displays the number of times the port transitioned from STP Learning to Forwarding state.