# Creating LLDP MED policies

Use this procedure to create a new LLDP MED policy for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, double-click Diagnostics.

3. In the Diagnostic tree, double-click 802.1AB.

4. In the 802.1AB tree, double-click Port MED.

5. In the work area, click the Local Policy tab.

6. Click Insert .

7. To select a port to create a policy for, click the PortNum elipsis.

8. Click Ok .

9. In the PolicyAppType section, select one or both boxes.

10. To select a VLAN identifier for the selected port, click the PolicyVlanID elipsis.

11. Click Ok .

12. Double-click the PolicyPriority box.

13. Type a priority value.

14. Double-click the PolicyDscp box.

15. Type a DSCP value.

16. To use a tagged VLAN, click the PolicyTagged box.

    OR

    To use an untagged VLAN, clear the PolicyTagged box.

17. Click Insert .

Use the data in the following table to create a new LLDP MED policy for the local system.

Table 1. Variable definitions
Field | Description
--- | ---
PortNum | Specifies the port on which to configure LLDP MED policies.
PolicyAppType | Specifies the policy application type. voice—selects the voice network policy voiceSignaling—selects the voice signaling network policy
PolicyVlanID | Specifies the VLAN identifier for the selected port or ports. Values range from 1–4094. If you select priority tagged frames, the system recognizes only the 802.1p priority level and uses a value of 0 for the VLAN ID of the ingress port.
PolicyPriority | Specifies the value of the 802.1p priority that applies to the selected switch port or ports. Values range from 0–7.
PolicyDscp | Specifies the value of the Differentiated Service Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475 that is associated with the selected switch port or ports. Values range from 0–63.
PolicyTagged | Specifies the type of VLAN tagging to apply on the selected switch port or ports. when selected—uses a tagged VLAN when cleared—uses an untagged VLAN or does not support port-based VLANs. If you select untagged, the system ignores the VLAN ID and priority values, and recognizes only the DSCP value.