# Configuring ECMP using EDM

Use the following procedure to configure and ECMP settings for RIP, OSPF, and static routes.

## Prerequisites

- Install the Advanced License.

- Enable IP routing globally on the switch.

- Configure routing (RIP, OSPF, or static routes) on the switch.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click IP.

3. In the work area, click the ECMP tab.

4. To select a protocol for which to configure ECMP, double-click the table cell in the MaxPath column heading for the protocol.

5. Type a value in the text box.

6. Repeat steps 4 and 5 as required.

7. On the toolbar, click Apply.

8. On the toolbar, you can click Refresh to verify the ECMP configuration.

## Variable definitions

The following table describes the fields of the ECMP tab.

Field | Description
--- | ---
RoutingProtocol | Indicates the routing protocol to be configured.
MaxPath | Indicates the maximum number of ECMP paths assigned to the protocol. Value ranges between 1 and 4. Default is 1.