# Downloading an ASCII configuration file from a USB device using EDM

## About this task

Use this procedure to download an ASCII configuration file from a USB device.

## Procedure

1. From the Navigation tree, double-click Edit.
2. From the Edit tree, double-click File System.
3. Select the Ascii Config File tab.
4. In TftpServerInetAddress, type the configuration file name.
5. In UsbTargetUnit, enter the stack unit number where the USB device is inserted.
6. In AsciiConfigManual-Download, click downloadFromUsb to transfer the file from the USB device to the switch.
7. On the toolbar, click Apply.