# Downloading a binary configuration file from a USB device using EDM

## About this task

Use this procedure to download a binary configuration file from a USB device.

## Procedure

1. From the Navigation tree, double-click Edit.
2. From the Edit tree, double-click File System.
3. Select the Config/Image/Diag File tab.
4. In BinaryConfigFilename, enter the configuration file name.
5. In UsbTargetUnit, enter the stack unit number where the USB is inserted.
6. In Action, click dnldConfigFromUsb.
7. On the toolbar, click Apply.