# Viewing topology information

To view topology information:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click Topology.

4. Select the Topology tab.

The following table outlines the parameters of the Topology tab.

Table 1. Variable definitions
Variable | Value
--- | ---
IpAddr | The IP address of the device.
Status | Whether Avaya topology is on (topOn) or off (topOff) for the device. The default value is topOn.
NmmLstChg | The value of sysUpTime the last time an entry in the network management MIB (NMM) topology table was added, deleted, or modified. If the table has not changed since the last cold or warm start of the agent, then the value is zero.
NmmMaxNum | The maximum number of entries in the NMM topology table.
NmmCurNum | The current number of entries in the NMM topology table.