# Modifying a VLAN

Use this procedure to modify a VLAN's name, member ports, or routing status without recreating the VLAN.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VALN tree, click VLANs.

3. Select the Basic tab.

4. To modify the VLAN name, double-click in the Name field.

5. To modify the Routing status, double-click in the Routing field and select from the drop-down list.

6. To modify VLAN member ports, in the row that represents the VLAN that is to be modified, double-click in the PortMembers field.

   The Port Members screen appears.

7. Click the buttons that correspond to the ports that are to be added or deleted from the VLAN. Click All to select all switch ports.

8. Click OK.

9. Click Apply.