# Displaying IPFIX data information

Use this procedure to set the display criteria and display IPFIX data information.

## Procedure steps

1. From the navigation tree, double-click Serviceability.

2. In the Serviceability tree, click IPFIX.

3. In the work area, click the Data Information tab.

## Variable definitions

Variable | Value
--- | ---
Unit Number | Specifies whether the switch is a standalone or part of a stack. A value of 1 indicates a standalone switch. A value greater than 1 indicates the switch location in a stack.
Sort By | Specifies a rule to sort the data. Values include: Source Address — source IP address Destination Address — destination IP address Protocol — protocol number TOS — type of service Port — port number TCP/UDP Src Port — TCP/UDP source port TCP/UDP Dst Port — TCP/UDP desitnation port Packet Count — packet number Byte Count — data byte number First Packet Time — first packet time Last Packet Time — last packet time
Sort Order | Specifies ascending or descending.
Display | Specifies the number of entries to display. Values include: Top 10 Top 25 Top 50 Top 100 Top 200