# Viewing remote 802.1Q Framing TLV information

Use this procedure to display Layer 2 frame tagging mode information received on switch ports from connected Avaya IP phones.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. In the Edit tree, click Diagnostics.

3. In the Diagnostics tree, click 802.1AB.

4. In the 802.1AB tree, click Avaya.

5. In the work area, click the Neighbor Dot1Q tab.

## Variable definitions

Variable | Value
--- | ---
TimeMark | Displays the time the latest TLV-based information is received from an Avaya IP phone.
LocalPortNum | Displays the number of the switch port on which the TLV-based information is received.
Index | Displays a unique identifier for the connected Avaya IP phone.
Dot1QFraming | Displays the Layer 2 frame tagging mode for the Avaya IP phone connected to the switch port. Values include: tagged—frames are tagged based on the tagging value the Avaya IP phone receives with the LLDP-MED Network Policy TLV. non-tagged—frames are not tagged with 802.1Q priority. auto—an attempt is made to tag frames based on the tagging value the Avaya IP phone receives with the LLDP-MED Network Policy TLV. If there is no LLDP-MED Network Policy information available, an attempt is made to tag frames based on server configuration. If that fails, traffic is transmitted untagged. The default tagging mode is auto.