# Configuring DHCP relay interface parameters

Configure the DHCP relay behavior on the interface.

## Procedure steps

1. From the navigation tree, double-click IPv6.

2. Double-click DHCP Relay.

3. In the Interface tab, click Insert.

4. Enter the appropriate values.

5. Click Insert.

## Variable definitions

The following table describes the fields of the Interface tab.

Variable | Value
--- | ---
IfIndex | A read-only value indicating the unique value to identify an IPv6 interface.
MaxHop | Specifies the maximum number of hops a DHCP packet can take from the DHCP client to the DHCP server.
RemoteIdEnabled | Enables or disables remote ID.