# Configuring stack units

Use the following procedure to configure stack units, and to display stack unit information.

## About this task

You can use the Stack Info tab to reset stack units, to enter a location for stack units, or to view stack unit status information.

## Procedure

1. From the navigation tree, double-click Edit.
2. In the Edit tree, double-click Chassis.
3. In the Chassis tree, click Switch/Stack.
4. In the work area, click the Stack Info tab.
5. In a unit row, double-click the Location cell and type a character string.
6. In a unit row, double-click the AdminState cell and select a value from the list.
7. On the toolbar, click Apply.

## Variable definitions

The following table describes configuring and displaying the stack unit status.

Variable | Value
--- | ---
Indx | Indicates the unique identifier number for the stack unit.
Descr | Indicates the stack unit port description.
Location | Specifies the physical location of the stack unit.
LstChng | Indicates the sysUpTime when the interface entered the operational state. If you entered the current state prior to the last reinitialization of the local network management subsystem, the value is zero.
AdminState | Specifies the administrative state of the stack unit. Values include enable or reset.
OperState | Indicates the operational state of the stack unit.
Ver | Indicates the stack unit hardware version.
SerNum | Indicates the stack unit serial number.
BaseNumPorts | Indicates the number of base ports on the stack unit.
TotalNumPorts | Indicates the total number of ports on the stack unit.
IpAddress | Indicates the stack unit IP address.
RunningSoftwareVer | Indicates the version of the running software.