# Enabling EAPOL multihost Fail Open VLAN using EDM

Use the following procedure to enable the EAPOL multihost Fail Open VLAN.

## Prerequisites

- Guest Vlan and failopen vlan do not have the same vid.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click 802.1X/EAP.

3. On the EAPOL tab, select the MultihostFailOpenVlanEnabled option.

4. On the toolbar, click Apply.

## Job aid

The following example procedure specifies the use of VoIP VLAN and Fail Open VLAN.

1. Specify VoIP VLANs. These must not be Fail Open VLANs or Guest VLANs on any port.

2. Specify Fail Open VLAN. This must not be VoIP VLANs or Guest VLANs on any port.

3. Specify Guest VLANs. These must not be VoIP VLANs or Fail Open VLANs.

4. Enable non-phone-enable on a specific port and globally.

5. Enable GuestVlan on the same port and globally.

6. Enable FailOpen globally.