# Configuring Link Aggregation Groups

Us this procedure to configure Link Aggregation Groups.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the LACP tab.

## Variable definitions

The following table outlines the parameters of the LACP tab.

Table 1. MLT/LACP LACP tab parameters
Variable | Value
--- | ---
Index | Specifies the unique identifier allocated to this Aggregator by the local System. This attribute identifies an Aggregator instance among the subordinate managed objects of the containing object. This value is read-only.
MacAddress | Specifies the MAC address used by this bridge when it must be referred to in a unique fashion.
AggregateOrIndividual | A read-only Boolean value indicating whether the Aggregation Port can Aggregate (TRUE) or can only operate as an Individual link (FALSE).
ActorLagID | Specifies the combined information of ActorSystemPriority, ActorSystemID, and ActorOperKey in ActorSystemPriority-ActorSystemID-ActorOperKey format.
ActorSystemPriority | A 2-octet read-write value indicating the priority value associated with the Actor's System ID.
ActorSystemID | Specifies a 6-octet read-only MAC address value that defines the value of the System ID for the System that contains this Aggregation Port.
ActorOperKey | Specifies the current operational value of the Key for the Aggregation Port. This is a 16-bit read-only value.
ActorAdminKey | Specifies the current administrative value of the Key for the Aggregation Port. This is a 16-bit read-write value.
PartnerLagID | Specifies the combined information of PartnerSystemPriority, PartnerSystemID, and PartnerOperKey in PartnerSystemPriority-PartnerSystemID-PartnerOper Key format.
PartnerSystemPriority | Specifies a 2-octet read-only value that indicates the priority value associated with the Partner's System ID.
PartnerSystemID | Specifies a 6-octet read-only MAC address value consisting of the unique identifier for the current protocol Partner of this Aggregator. A value of zero indicates that no known Partner exists. If the aggregation is manually configured, this System ID value is assigned by the local System.
PartnerOperKey | Specifies the current operational value of the Key for the Aggregator's current protocol Partner. This is a 16-bit read-only value.
CollectorMaxDelay | Specifies the value of this 16-bit read-write attribute defines the maximum delay, in tens of microseconds, that can be imposed by the Frame Collector between receiving a frame from an Aggregator Parser, and either delivering the frame to its MAC Client or discarding the frame.