# Storing the current ASCII configuration file on a USB device using EDM

## About this task

Use this procedure to save the current ASCII configuration file on a USB device.

## Procedure

1. From the Navigation tree, double-click Edit.
2. From the Edit tree, double-click File System.
3. Select the Ascii Config File tab.
4. In TftpServerInetAddress, type the configuration file name.
5. In UsbTargetUnit, enter the stack unit number where the USB device is inserted.
6. In AsciiConfigManualUpload, click uploadToUsb.
7. On the toolbar, click Apply.