# Viewing LLDP local system properties

With the Local System tab, you can view LLDP properties for the local system.

To view LLDP local system properties:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click LLDP.

5. Select the Local System tab.

The following table outlines the parameters of the LLDP Local System tab.

Table 1. Variable definitions
Variable | Value
--- | ---
ChassisIdSubtype | the type of encoding used to identify the local system chassis: chassisComponent interfaceAlias portComponent macAddress networkAddress interfaceName local
ChassisId | chassis ID
SysName | local system name
SysDesc | local system description
SysCapSupported | identifies the system capabilities supported on the local system
SysCapEnabled | identifies the system capabilities that are enabled on the local system
DeviceClass | local MED device class
HardwareRev | the vendor-specific hardware revision string as advertised by the local device
FirmwareRev | the vendor-specific firmware revision string as advertised by the local device
SoftwareRev | the vendor-specific software revision string as advertised by the local device
SerialNum | the vendor-specific serial number as advertised by the local device
MfgName | the vendor-specific manufacturer name as advertised by the local device
ModelName | the vendor-specific model name as advertised by the local device
AssetID | the vendor-specific asset tracking identifier as advertised by the local device
DeviceType | defines the type of Power-via-MDI (Power over Ethernet) advertised by the local device: pseDevice: indicates that the device is advertised as a Power Sourcing Entity (PSE). pdDevice: indicates that the device is advertised as a Powered Device (PD) none: indicates that the device does not support PoE
PSEPowerSource | defines the type of PSE Power Source advertised by the local device: primary: indicates that the device advertises its power source as primary backup: indicates that the device advertises its power source as backup
PDPowerReq | specifies the value of the power required (in units of 0.1 watts) by a Powered Device (PD)
PDPowerSource | defines the type of power source advertised as in use by the local device: fromPSE: indicates that the device advertises its power source as received from a PSE local: indicates that the device advertises its power source as local localAndPSE: indicates that the device advertises its power source as using both local and PSE power
PDPowerPriority | defines the priority advertised as required by this PD: critical: indicates that the device advertises its power priority as critical, see RFC 3621 high: indicates that the device advertises its power priority as high, see RFC 3621 low: indicates that the device advertises its power priority as low, see RFC 3621