# Configuring meter capability filtering

Use this procedure to configure Meter Capability filtering.

## Procedure steps

1. From the navigation tree, double-click QoS.

2. From the QoS tree, double-click QoS Devices.

3. Select the Meter Capability tab.

4. Click the Filter button to set Meter Capability table view filtering criteria.

   The QOSDevice, Meter Capability - Filter dialog opens.

5. Select filtering criteria and enter port, meter support, and meter rate parameters.

6. To activate your selections, click the Filter button on the dialog, the Meter Capability window will display entries based on the filtering criteria specified.

For more information, see Table 1.