# Configuring Global IPFIX

IPFIX functionality can be globally enabled or disabled from the EDM. By default, IPFIX is disabled and you must enable it before it starts to collect flow information. This section contains the procedures for enabling and disabling IPFIX on a switch.

Use the following command to enable or disable IPFIX.

## Procedure steps

1. From the navigation tree, double-click Serviceability.

2. In the Serviceability tree, click IPFIX.

3. In the Global tab work area, select the operational state of IPFIX functionality in the State area.

4. In the toolbar, click Apply.