# Viewing VLACP Global information

Use this procedure to view VLACP information for the switch.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click MLT/LACP.

3. Select the VLACP Global tab.

## Variable definitions

The following table outlines the parameters of the VLACP Global tab.

Table 1. MLT/LACP VLACP Global tab parameters
Variable | Value
--- | ---
Enable | Enables or disables VLACP on the switch.
MulticastMACAddress | Identifies a multicast MAC address used exclusively for VLACPDUs. Default is 01:80:c2:00:11:00.