# Configuring Security list using EDM

This section describes the procedure you can use to configure the security list to manage the port members in a security list.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Adding ports to a security list using EDM

Use the following procedure to insert new port members into a security list.

### Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click MAC Security.

3. In the work area, click the SecurityList tab.

4. In the toolbar, click Insert.

   The Insert SecurityList dialog box appears.

5. In the SecurityListIndx box, type a number for security list.

6. Click the SecurityListMembers ellipsis (...).

7. In the SecurityListMembers dialog box, select ports to add to the security list.

   OR

   Click All to select all ports.

8. Click Ok.

9. Click Insert.

### Variable definitions

Use the data in the following table to add ports to the security list.

Variable | Value
--- | ---
SecurityListIndx | Indicates the numerical identifier for a security list. Values range from 1 to 128.
SecurityListMembers | Defines the security list port members.

## Deleting specific ports from a security list using EDM

Use the following procedure to remove specific existing port members from a security list.

### Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click MAC Security.

3. In the work area, click the SecurityList tab.

4. In the table, double-click the cell under the SecurityListMembers column heading.

5. Clear the port members you want to remove from the list.

6. Click Ok.

7. In the toolbar, click Apply.

### Variable definitions

Use the data in the following table to delete specific ports from a security list.

Variable | Value
--- | ---
SecurityListIndx | A numerical identifier for a security list. Values range from 1 to 128.
SecurityListMembers | Defines the security list port members.

## Deleting all ports from a security list using EDM

Use the following procedure to remove all existing port members from a security list.

### Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click MAC Security.

3. In the work area, click the SecurityList tab.

4. Select the security list you want to delete.

5. In the toolbar, click Delete.

6. Click Yes to confirm.

### Variable definitions

Use the data in the following table to delete all ports from a security list.

Variable | Value
--- | ---
SecurityListIndx | A numerical identifier for a security list. Values range from 1 to 128.
SecurityListMembers | Defines the security list port members.