# Configuring Auto Unit Replacement

Use the following procedure to configure Auto Unit Replacement (AUR).

## Procedure

1. From the navigation tree, double-click Edit.
2. In the Edit tree, double-click Chassis.
3. In the Chassis tree, click Chassis.
4. In the work area, click the AUR tab.
5. To enable AUR, select the AutoUnitReplacementEnable check box. To disable AUR, clear the check box.
6. To enable AUR configuration saves, select the AutoUnitReplacementSaveEnabled check box. To disable AUR saves, clear the check box.
7. In the AutoUnitReplacementForceSave field, type a value.
8. In the AutoUnitReplacmentRestore field, type a value.
9. On the toolbar, click Apply.

## Variable definitions

The following table describes configuring Auto Unit Replacement.

Variable | Value
--- | ---
AutoUnitReplacementEnabled | Specifies if AUR is enabled or disabled. Check to enable, clear to disable.
AutoUnitReplacementSaveEnabled | Specifies if AUR automatic saves of unit configuration images is enabled or disabled. Check to enable, clear to disable.
AutoUnitReplacementForceSave | Specifies to manually save a specific non-base unit configuration image to the base unit. Value range of 0 to 8.
AutoUnitReplacementRestore | Specifies to manually restore the configuration of a specific non-base unit from the saved configuration image on the base-unit. Value range of 0 to 8.