# Viewing LLDP Neighbor Protocol VLAN properties

With the Neighbor Protocol VLAN tab, you can view LLDP Protocol VLAN properties for the remote system.

To view the Neighbor Protocol VLAN tab:

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port dot1.

5. Select the Neighbor Protocol VLAN tab.

The following table outlines the parameters of the Port dot1 Neighbor Protocol VLAN tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | The TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | An arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
ProtoVlanId | The ID of the port and protocol VLANs associated with the remote port. A value of zero is used if the system does not know the protocol VLAN ID (PPVID).
ProtoVlanSuported | Indicates whether the remote port supports port and protocol VLANs.
ProtoVlanEnabled | Indicates whether the port and protocol VLANs are enabled on the remote port.