# Creating a multicast-static IP routing table entry

Use this procedure to create an entry in the multicast-static IP routing table.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click IP.

3. In the IP work area, click the Static MRoutes tab.

4. On the toolbar, click Insert.

5. Configure the parameters as required.

6. Click Insert.

## Variable definitions

Variable | Value
--- | ---
IpAddressType | Specifies the type of IP Address (ipv4).
IpAddress | Specifies the IP address of the destination network.
Mask | Specifies the mask of the destination network.
RpfAddressType | Specifies the type of address for the reverse path forwarding address (ipv4).
RpfAddress | Specifies the reverse path forwarding address.
Preference | Specifies the administrative distance of the static multicast route