# Configuring NSNA static clients using EDM

Use the following procedure to configure NSNA static clients.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

Static clients must have their MAC address registered in the SNAS 4050 MAC database and they must be members of an SNAS 4050 group that uses MAC authentication (mactrust set to bypass). For more information, see Secure Network Access Switch 4050 User Guide for ACLI , NN47230-100.