# Configuring SLPP PDU transmit interval

Use this procedure to configure the SLPP PDU transmit interval in milliseconds.

## Procedure steps

1. From the navigation tree, double-click VLAN.

2. From the VLAN tree, click SLPP.

3. Select the Global tab.

4. In the TransmissionInterval text box, enter the value, in milliseconds, for the transmit interval in the range 500 to 5000. The default is 500.

5. Click Apply.

6. Click Close.