# Viewing information about NSNA clients using EDM

Use the following procedure to view information about NSNA clients currently connected to the network access device.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click NSNA.

3. In the work area, select the Nsna Client tab to view the clients currently connected to the network access device.

## Variable definitions

The following table describes the Nsna Client fields.

Variable | Value
--- | ---
IfIndex | Specifies the ifIndex of the port on which the client is attached.
MacAddress | Specifies the MAC address of the client.
Device Type | Specifies the type of client device (pc, ipPhone, or a passive device).
VlanId | Specifies the VLAN ID of the client.
FilterVlanId | Specifies the VLAN ID whose associated filter set is installed in the selected port.
AddressType | Specifies the type of IP address used by this client (IPv4 is currently the only option available).
Address | Specifies the IP address of the client.
Expired | Indicates whether this client has been aged-out.