# Viewing LLDP remote management properties

Use this procedure to view LLDP management properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the Neighbor Mgmt Address tab.

The following table outlines the parameters of the Neighbor Mgmt Address tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Identifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
AddrSubtype | Specifies the type of encoding used in the associated Addr object.
Addr | Identifies the management address associated with the remote system.
AddrIfSubtype | Identifies the numbering method used to define the interface number associated with the remote system. unknown ifIndex systemPortNumber
AddrIfId | Identifies the interface number of the management address component associated with the remote system.
AddrOID | Identifies the type of hardware component or protocol entity associated with the management address advertised by the remote system agent.