# Displaying LLDP transmit statistics

Use this procedure to view LLDP transmit statistics by port.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click LLDP.

5. Select the TX Stats tab.

The following table outlines the parameters of the TX Stats tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
FramesTotal | Specifies the number of LLDP frames transmitted by this LLDP agent on the indicated port.