# Viewing local location properties

Use this procedure to view LLDP location properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Local Location tab.

The following table outlines the parameters of the Port MED Local Location tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
LocationSubtype | Specifies the location subtype advertised by the remote device: unknown coordinateBased civicAddress elin
LocationInfo | Specifies the location information. The parsing of this information is dependent on the value LocationSubtype.