# Viewing LLDP local PoE PSE properties

Use this procedure to view LLDP PoE PSE properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Local PoE PSE tab.

The following table outlines the parameters of the Port MED Local PoE PSE tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Specifies the port number.
PSEPortPowerAvailable | Specifies the value of the power available (in units of 0.1 watts) from the PSE through this port.
PSEPortPDPriority | Indicates the PD power priority that is advertised on this PSE port: unknown: priority is not configured or known by the PD critical: the device advertises its power priority as critical, see RFC 3621 high: the device advertises its power priority as high, see RFC 3621 low: the device advertises its power priority as low, see RFC 3621