# Viewing LLDP Neighbor Protocol properties

Use this procedure to view LLDP Protocol properties for the remote system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, click Port dot1.

5. Select the Neighbor Protocol tab.

The following table outlines the parameters of the Neighbor Protocol tab.

Table 1. Variable definitions
Variable | Value
--- | ---
TimeMark | Specifies the TimeFilter for this entry.
LocalPortNum | Identifies the local port on which the remote system information is received.
Index | Specifies an arbitrary local integer value used by this agent to identify a particular MSAP. An agent is encouraged to assign monotonically increasing index values to new entries, starting with one, after each reboot.
ProtocolIndex | Represents an arbitrary local integer value used by this agent to identify a particular protocol identity.
ProtocolId | Identifies the protocols associated with the remote port.