# Viewing local policy properties

Use this procedure to view LLDP policy properties for the local system.

## Procedure steps

1. From the navigation tree, double-click Edit.

2. From the Edit tree, double-click Diagnostics.

3. From the Diagnostics tree, double-click 802.1AB.

4. From the 802.1AB tree, double-click Port MED.

5. Select the Local Policy tab.

6. Click Insert. The Insert Local Policy dialog box appears.

7. Enter the parameters according to the Variable definitions table.

8. Click Insert.

The following table outlines the parameters of the Port MED Local Policy tab.

Table 1. Variable definitions
Variable | Value
--- | ---
PortNum | Identifies the port number.
PolicyAppType | Specifies voice or voice-signaling application type.
PolicyVlanID | An extension of the VLAN Identifier for the port, as defined in IEEE 802.1P-1998. A value of 1 through 4094 is used to define a valid PVID. A value of 0 is used if the device is using priority tagged frames, meaning that only the 802.1p priority level is significant and the default VID of the ingress port is being used instead. A value of 4095 is reserved for implementation use.
PolicyPriority | Indicates the value of the 802.1p priority which is associated with the local port.
PolicyDscp | Specifies the value of the Differentiated Service Code Point (DSCP) as defined in IETF RFC 2474 and RFC 2475 that is associated with the given port on the local system.
PolicyTagged | A value of true indicates that the application is using a tagged VLAN. A value of false indicates that for the specific application, the device is using an untagged VLAN or does not support a port based VLAN operation. In this case, both the VLAN ID and the Layer 2 priority fields are ignored, and only the DSCP value has relevance.