# Viewing brouter port and VRF associations

Use this procedure to view each port and associated VRFs. You can also change the VRFs associated with the port if the port has no IP address.

## Procedure steps

1. From the navigation pane, double-click IP.

2. In the IP tree, click VRF.

3. In the VRF work area, click the VRF-Ports tab.

4. To change the VRF, double-click the BrouterVrfId field for the port.

   Tip

   You can associate a port with more than one VRF.

5. Choose the required VRFs, and click Ok.

6. Click Apply.

## Variable definitions

Variable | Value
--- | ---
rcPortIndex | Specifies the port number.
Type | Specifies the port type.
BrouterVrfId | Specifies the VRF ID for this brouter port.
BrouterVrfname | Specifies the VRF name for this brouter port.