# Job aid, folders and subfolders in the navigation tree

Table 1. Job aid, folders and subfolders in the navigation tree
Folder | Description
--- | ---
Administration | Use the tabs associated with the sub-folders in the Administration folder to perform the following functions: Quick Start –set up IP/Community/Vlan and Trap Receiver Remote Access – enable or disable Telnet, SNMP, Web Page, and SSH MIB Web Page – perform a MIB Walk
Device | Rediscover Device—Use the Rediscover Device selection to refresh the session. Caution: all existing tabs are lost
Edit | Use the tabs associated with the sub-folders in the Edit folder to view or change parameters for the currently-selected object. Sub-folders in the Edit folder are Unit Chassis: Chassis, Switch/Stack, ports, and environment Bridge File System ADAC Diagnostics: Port Mirrors, Topology, System Log. 802.1AB: LLDP, Port dot1, Port dot3, Port MED SNTP/Clock Snmp Server: MIB View, User, Community, Host, Notification Control
Security | Use the tabs associated with the sub-folders in the Security folder to view or change security settings. Sub-folders in the Security folder are MAC Security DHCP Snooping Dynamic ARP Inspection (DAI) IP Source Guard (IPSG) 802.1X/EAP Web/Telnet/Console SSH/SSL RADIUS NSNA TACACS+
Graph | Use the tabs associated with the sub-folders in the Graph folder to view statistics and produce graphs of the statistics. Sub-folders in the Graph folder are Chassis Port—to view or graph statistics for a port, first select a port on the Device Physical View.
Power Management | Use the tabs associated with the sub-folders in the Power Management folder to view and configure Power over Ethernet (PoE) settings and to view and configure Energy Saver settings. Sub-folders in the Power Management folder are PoE Energy Saver PoE is only available for switches equipped with Power over Ethernet.
VLAN | Use the tabs associated with the sub-folders in the VLAN folder to configure or view information about VLANs, Spanning Tree, and Multi-Link Trunking. Sub-folders in the VLANs folder are VLANs Spanning Tree: Globals, STG, RSTP, MSTP MLT/LACP SLPP
IP Routing | Use the tabs associated with the sub-folders in the IP Routing folder to configure IP routing functions. Sub-folders in the IP Routing folder are IP TCP/UDP OSPF RIP VRRP Multicast IGMP PIM DHCP UDP Forwarding Policy
IPv6 | Use the tabs associated with the sub-folders in the IPv6 folder to set up IPv6 routing functions. Sub-folders in the IPv6 folder are IPv6 TCP/UDP Tunnel DHCP Relay
QoS | Use the tabs associated with the sub-folders in the QoS folder to configure quality of service and set up QoS policies and filters. Sub-folders in the QoS folder are QoS Devices QoS Rules QoS QoS Agent QoS NSNA/UBP/Traffic Profile
Serviceability | Use the tabs associated with the sub-folders in the Serviceability folder to monitor traffic flows using IPFIX, and to monitor and configure remote monitoring. Sub-folders in the Serviceability folder are IPFIX RMON: Alarms, Control